Inflatable start up:

**PLEASE DO NOT SET UP INFLATABLE IF WINDS ARE STRONGER THAN 10 MPH!! Use the wind gauge provided to check wind speed.**

One person is responsible to read the instructions step by step as others put up and take down the inflatable. When putting inflatable back in trailer please roll in backwards on handtruck, leave standing up on the handtruck. Attach to the wall of the trailer with the straps provided. IF the inflatable is not cleaned, dried, rolled up, and replaced in the proper position once returned, the church or ministry will be asked to unload and redo it. This is for the protection of the inflatable as well as for the next ministry that uses it to see how it is to be left when they deliver it back to the CBA. Thank you for your understanding in this matter.

1. Before beginning this process, watch the video found at centennialbaptistassociation.com/outreachtrailer that is entitled “Inflatable startup.” Additional information can be found in the notebook containing Jungle Jumps Setup, Operation, and Maintenance Manual.
2. At least two adults are needed to ensure safety when moving the inflatable.
3. Detach inflatable from the wall of the trailer, but leave strapped to the handtruck. Leave straps attached to the wall for safe-keeping.
4. Slowly tilt inflatable on the handtruck with one person in front and the other behind. Roll gently out the back of the trailer.
5. DO NOT drag the inflatable on grass or pavement.
6. Once at the location stand the handtruck up and untie the inflatable.
7. Check the ground for any debris including rocks, sticks, or sharp objects that may damage the inflatable.
8. Spread out the tarp to cover all of the ground area, leaving the excess (appx. 1 ½ feet) on three sides and the rest (appx. 10 feet) on the entrance/exit side. Use orange-topped tent pegs to secure tarp to the ground.
9. Unfold the inflatable. NOTE: the two air flow “legs” are on the back side of the inflatable.
10. Take the blower and place one of the back air flow “legs” around the mouth of the blower and strap it tight.
11. Take the end of the second air flow “leg” and fold over and wrap the strap around it and pull tight. You may have to make two or three folds to have enough to pull the strap tight. (Please make sure that the strap buckle does not rub against the air flow leg.)
12. Hook up the power cords to the blower and push the start button. If you need an extension cord, use the 12 gauge heavy duty cords provided in the Outreach Trailer.
13. Once the inflatable is up, find the four corner straps. Pull these outward till tight and using the small sledge hammer, nail spikes into the ground. If the ground it too hard or you are using the bounce house indoors, use two sandbags for each tie-down.
14. Finally make sure that the entire inflatable is on top of the tarps before use.
15. During use there should be at least two people manning the inflatable assisting the entering and the exits of those playing. Also take note of the number of people allowed which is printed on the inflatable.

**Safety Rules**

**Check with your local government for any specific rules related with moonwalk safety.**

* Before the inflatable unit is securely anchored and fully inflated, do not allow anybody to get inside or on the inflatable.
* In case of power failure, empty the moonwalk immediately.
* Do not use in high wind, rain, snow or lightning conditions. If wind exceeds 15 MPH, empty the inflatable and deflate the inflatable.
* Use an adequate three wire extension cord, min. 12 gauge for 50ft. Never cut or remove the round grounding pin from the cord. Check with your local regulation and blower's manufacturer user manual for the use of the blower and the extension cord.
* Always connect a GFI extension cord adaptor to any extension cord before plugging into a power source to reduce the possibility of shock in damp environments.
* Check the GFI operation at least once per event.
* Check the connection of GFI extension cord and any extension cord frequently when using the inflatable.
* Do not allow anybody to carry sharp objects while playing in the inflatable
* Do not allow anybody inside the bounce house or get on the slide before the inflatable is fully inflated.
* Get the map of underground utilities before driving in any stakes
* Do not allow any children or adults in the rear of the ride or near the blower at any time.
* **No head-down play on any inflatable amusement devices.** No play or jump on the safety step or near the entrance/exit. No head-down slide on any slide or safety step. No play or jump on the top platform of any slide.
* Ground stakes should follow the specification stated in this manual. If the ground is loose, use longer stakes accordingly. Cover the stake heads properly to avoid falling. Check regularly to ensure they are tight when the inflatable is in use.
* No children 3 years old and under, or less than 42" tall allowed to use any of the inflatable devices.
* Do not put fingers or hands into blower when running.
* Always leave enough space around and above the inflatable.
* Use proper barriers to prevent crowds to move close to the inflatable device other than the designated area such as entrance and exit.

**Deflation and Packing Instructions**

1. Inspect both inside and outside for any damage.
2. Clean and dry! Sweep or vacuum the inside of the inflatable. Use only the Simple Green and Odo-ban provided and clean all surfaces that would be in contact with children (floor, entrance, walls). Never use degreaser or bleach on the inflatable. Use shop towels to dry everything before deflating to avoid mildew.
3. Do not allow any children or adults inside or in the rear of the inflatable.
4. Turn the blower off and unplug the blower from power source.
5. Untie the strap of the air tube from the blower. Lay the air tube flat to let the air out. Untie the other air tube, if there is one.
6. Remove stakes and extension cords.
7. You may walk with bare feet on the deflated inflatable unit from front towards the air tubes to let out more air.

**Folding Process**

1. Check to make sure the inflatable is clean and dry both inside and outside.
2. Place the inflatable as flat as possible. Fold in outside walls, base of the inflatable, step, cartoon character towards the middle of the unit. Leaving the bottom edge of the inflatable as the edge.
3. Prior to rolling, make sure at least one of the air tubes is able to let more air out at your rolling process.
4. Fold one-fourth of the inflatable in, and fold in one-fourth from the other side.
5. Fold one part over the other part. Step on the inflatable to let out more air. Begin rolling the inflatable from front end to back end. Be sure the roll is straight and tight at the very beginning of the rolling, and at all the rolling process.
6. Near the end of the inflatable, slow down to let out more air. When reach the end of the inflatable, roll back a little bit and fold in the remaining air tubes.
7. Use straps to tie tight around the roll.
8. Tilt the inflatable to an upright position and place it on the handtruck. Strap the inflatable to the handtruck
9. Take the blue tarp and fold it into a square and place between the red lines in the bottom of the trailer over the axle. This will assure that the inflatable is protected from rubbing on the floor during transport.
10. Walk the handtruck up the back ramp of the trailer and carry the front of the inflatable to where you laid the blue tarp.